

TIM-1000

S/W Release Notes

|  |  |  |  |
| --- | --- | --- | --- |
|  | Name | Position | Date |
| Prepared By | Ravindra Parmar | Product Manager | 11/05/20 |
| Approved By | Jim Hallington | Managing Director | 11/05/20 |

# Introduction

The document describes the release of TIM-1000 software version 2.7

# Contents of Release

* Clockaudio\_Mic-Array\_release-notes\_2.5.docx – these release notes
* installer-2.7.tar.signed.tar – the update file

# Change History

## v2.4.2 (29/05/2018)

* Initial release

## v2.5 (31/07/2019)

* Fix bounding box area around colour wheel selection

## v2.6 (31/12/2019)

* Reduce the amount of noise suppression by 3dB
* Readjust the EQ settings

## V2.7 (11/05/20)

* Rename APT’s “Normal” to “Max” and Set as default
* Introduce Presets functionality on GUI and add corresponding UDP commands (SLEDSTATE and GLEDSTATE)
* Secondary unit uses Main unit as NTP server
* Bug Fix: Dante IP address resets to DHCP after factory reset
* Bug Fix: EQ settings box spills out of bounding box for some screen resolutions

# Known issues

* Performing a factory reset on units that had pre-V2.7 code installed as factory image will not revert the Dante IP address to DHCP. If the Dante IP address was set as a static IP address, it will retain it.

# Instructions

Go to the Advanced tab (password is ‘clockaudio’ by default). There you should be able to drag and drop the “installer-2.7.tar.signed.tar” onto the “update” panel. Wait for the install to complete and TIM-1000 will automatically reboot into the new software.